**Alfa Romeo 4C**

**Colour:** Metallic Alfa Red

**Registration:** ES 885 VB

**Base Price:** €69,900

**TECHNICAL SPECIFICATION**

|  |  |
| --- | --- |
| **ENGINE** | |
| Type | 1750, all-aluminium, 4-cylinder, direct injection, turbocharged |
| Position / Orientation | Central / Transverse |
| Displacement (cm³) | 1,742 |
| Maximum power hp @ rpm | 240 @ 6000 |
| Maximum torque Nm @ rpm | 350 @ 2200 - 4250 |
| **DRIVING MODE SELECTOR** | |
| Type | Evolved Alfa D.N.A. |
| Positions | All Weather, Natural, Dynamic, Race |
| **TRANSMISSION** | |
| Gearbox | ALFA TCT dual dry-clutch, paddle controls and Launch Control |
| Number of gears | 6 + R |
| Drive | RWD, Electronic Q2 differential |
| **CHASSIS** | |
| Type | Carbon fibre monocoque, 2 seat coupé configuration |
| Front suspension | Double wishbone |
| Rear suspension | Evolved MacPherson |
| Front brakes (mm) | Dual-cast, perforated, ventilated, 305x28 discs with 4-piston Brembo® calipers |
| Rear brakes (mm) | Perforated, ventilated 292x22 discs |
| Standard tyres | (F) 205/45 R17 (R) 235/40 R18 |
| **STEERING** | |
| Steering box | Rack and pinion, unassisted |
| **PERFORMANCE** | |
| Acceleration 0-100 km/h | 4.5s |
| Braking distance 100-0 km/h | 36m |
| Top speed km/h | 257 |
| Max braking deceleration (g) | 1.25 |
| Max lateral acceleration (g) | 1.1 |
| **CAPACITIES - WEIGHTS** | |
| Unladen weight (kg) | 895 |
| Fuel tank (litres) | 40 |
| **FUEL ECONOMY AND EMISSIONS** | |
| Urban cycle l/100km | 9.8 |
| Extra-urban cycle l/100km | 5.0 |
| Combined cycle l/100km | 6.8 |
| CO2 emissions (g/km) | 157 |
| Environmental classification | Euro 6 |
| **DIMENSIONS** | |
| Length x Width x Height (mm) | 3989 X 1864 X 1183 |
| Wheelbase (mm) | 2380 |
| Luggage capacity (dm³) | 110 |